****************************************************************************

     README.TXT for Serial Touch Panel Driver Windows2000/XP

     Copyright(C) 2004 Fujitsu Component Ltd.  All rights reserved.

****************************************************************************

Index:
  1. Driver installation process

  2. Driver uninstall process

  3. Attention in use of a Touch panel driver

----------------------------------------------------------------------------

1. Driver Installation process
   
   Choose the thing that a Windows version fitted the touch panel used in the way
   of installing the following, and install a driver.

  [For Windows2000] 
   (1) When PC starts, "New Hardware Wizard" runs automatically. 
   (2) Click "Next>" button.  
   (3) Select "Don't search I will choose this driver to install".
   (4) Click "Have Disk..."
   (5) Click "Browse".
   (6) Specify Touch Panel Driver disk.
   (7) And click "Next>" button. 
   (8) It is confirmed that "Fujitsu Touch Panel Driver (Windows2000/XP)" was detected.
       And Click "Next>" button.
   (9) It is informed of the normality end of the installation.
       Click "OK" button.
   (10) Click "Finish" button. 

  [For WindowsXP] 
   (1) When PC starts, "Welcome to the Found New Hardware Wizard" runs automatically. 
   (2) Select "Install from a list or specific location(Advanced)".
       And click "Next>" button.  
   (3) Select "Don't search I will choose  this driver to install".
   (4) Click "Have Disk..."
   (5) Click "Browse".
   (6) Specify Touch Panel Driver disk.
   (7) And click "Next>" button. 
   (8) It is confirmed that "Fujitsu Touch Panel Driver (Windows2000/XP)"was detected. 
       And Click "Next>" button.
   (9) It is informed of the normality end of the installation.
       Click "OK" button.
   (10) Click "Finish" button. 
   
   Attention:

    * The driver do not work correctly. Please install Internet Explorer4.0 or more.
    * You must have Administrator's authority to install this driver.
    * if "New Hardware Wizard" does not run, touch panel device was installed as 
      "Standard Serial Mouse". In the case, please install as follows.
       (1) Run the "Setup.exe" file.
       (2) Click "Yes" button.
       (3) It is informed of the normality end of the installation.
           Click "OK" button.
    * When more than one touch panel connect in Windows2000.
      Restart is necessary when it is installed at the same time. 
    * This driver doesn't set up "Use Port" at the time of the installation. 
      Therefore, Touch panel doesn't work. Set up "Use port" after the installation. 
      Please set up as follows.
       (1) Open "Control panel" of the system.
       (2) Double click "Touch Panel" icon.
       (3) Open "Dual monitor Set-up" page.
       (4) Set up the port of the touch panel in "Use port". Only the port that this 
           driver finds a touch panel can be set up. 
       (5) Click "OK" button.


2. Driver uninstall process
   (1) Open "Control panel" of the system.
   (2) Double click "Add/Remove Programs" icon.
   (3) Select "Fujitsu Touch Panel Driver (Windows2000/XP)".
   (4) Click "Add/Remove" button.
   (5) Click "Yes" button at delete confirmation dialog box.
   (6) Driver uninstall process finishes successfully.
   (7) Restart the system.

3. Attention in use of a Touch panel driver

* Only the user whose account type is Administrator account can install or uninstall
  Touch Panel driver.
* Don't uninstall Touch Panel driver when two or more users are logging in the computer.
* The installation of this driver is necessary in each port. Therefore Plug and Play
  Touch Panel driver may stop working when a port is changed after the installation.
  Install a driver in that port again in that case.
* When the connection port (Serial connector) of the device is changed. Change it under the condition 
  which the power off of the PC. Right after Plug and Play device install. Problem may occur in the 
  system when a port is changed with the power on of the PC. 
